Chris Paro

Problem 3

1. Virtual int setDirection(GPIO\_DIRECTION) is a function that is used to define the direction of a GPIO pin to either an input or an output. setDirection is a case statement that points to the pins directory folder. The value inside the case statement is then written in the direction file.
2. GPIO\_VALUE.getValue() is a function that will read a GPIO pin and will then return the value that it reads from the pin.